**EventTimer 10:00**

***Sequences:***

* Beamer HDMI 1 (PPP view)
* Audio Mix Profile ‚Diashow‘
* HDMI Switch channel 1 (Laptop PPP)
* Start Backup Recorder
* Slidershow + Countdowntimer until eventtime reached or Pause if time < current time

***Information for technician:* T**

***Execution text for PPP:***

JokiAutomation.exe "Timer" "10:00"

**EventTimer Pause Text 1 Text 2**

***Sequences:***

* Beamer HDMI 1 (PPP view)
* Audio Mix Profile ‚Diashow‘
* HDMI Switch channel 1 (Laptop PPP)
* Slidershow + Pause, Text 1 and Text 2

***Information for technician:* P**

***Execution text for PPP:***

JokiAutomation.exe "Pause" "Urheberrechtlich keine Liveübertragung" "Es geht in Kürze weiter"

**Band**

***Sequences:***

* Beamer HDMI 1 (PPP view)
* Audio Mix Profile ‘Band’
* HDMI Switch channel 1 (Laptop PPP)

***Information for technician:* L**

***Execution text for PPP:***

JokiAutomation.exe "Band"

**GoPro Actioncamera**

***Sequences:***

* Audio Mix Profile ‘Gottesdienst’
* HDMI Switch channel 2 (GoPro)

***Information for technician:* G**

***Execution text for PPP:***

JokiAutomation.exe "GoPro"

**Camcorder 1 (cam with position controller)**

***Sequences:***

* Audio Mix Profile ‘Gottesdienst’
* HDMI Switch channel 3 (camcorder with position control)

***Information for technician:* A**

***Execution text for PPP:***

JokiAutomation.exe "Altar"

**Camcorder 2 (preacher view)**

***Sequences:***

* Audio Mix Profile ‘Predigt’
* HDMI Switch channel 4 (camcorder 2 preacher view)

***Information for technician:* K**

***Execution text for PPP:***

JokiAutomation.exe "Predigt"

**Prayer (prayer view)**

***Sequences:***

* Audio Mix Profile ‘Text’
* HDMI Switch channel 5 (combination PPP and GoPro)
* Beamer HDMI 1

***Information for technician:***  **G**

***Execution text for PPP:***

JokiAutomation.exe "Gebet"

**Beamer PPP View**

***Sequences:***

* Switch beamer to HDMI 1 (Laptop PPP view)

***Information for technician:* BP**

***Execution text for PPP:***

JokiAutomation.exe "BEAMER\_PPP"

**Beamer Livestream - View**

***Sequences:***

* Switch beamer to HDMI 2 (Livestream - view)

***Information for technician:***  **BS**

***Execution text for PPP:***

JokiAutomation.exe "BEAMER\_LiveStream"

**Beamer Videoclip Text 1 Text 2**

***Sequences:***

* Beamer analog input
* Audio Mix Profile ‚Diashow‘
* HDMI Switch channel 1 (Laptop PPP)
* Pause, Text 1 and Text 2

***Information for technician:* BA**

***Execution text for PPP:***

JokiAutomation.exe "BEAMER\_VideoClip" "Urheberrechtlich keine Liveübertragung" "Es geht in Kürze weiter"

**Beamer mute / demute**

***Sequences:***

* mutes / demotes the Beamer

***Information for technician:***  **BM**

***Execution text for PPP:***

JokiAutomation.exe "BEAMER\_Mute"

**Backup-Recorder Stop**

***Sequences:***

* stops the backup-recorder

***Information for technician:***  **RS**

***Execution text for PPP:***

JokiAutomation.exe "Backup\_Stop"

**shut down sequence**

***Sequences:***

* Stop backup recorder
* Switch off Beamer
* Switch off HDMI switch
* Switch off backup recorder
* Shut down raspberry pi

***Information for technician:***

**Ausschaltsequenz!!!**

***Execution text for PPP:***

JokiAutomation.exe  "Ausschaltsequenz"