**EventTimer 10:00**

***Sequences:***

* Beamer HDMI 1 (PPP view)
* Audiochannel 1 fade up
* Audiochannel 2,3,4 fade down
* HDMI Switch channel 1 (Laptop PPP)
* Slidershow + Countdowntimer until eventtime reached or Pause if time < current time

***Information for technician:***

1 B1 A1

***Execution text for PPP:***

JokiAutomation.exe "Timer" "10:00"

**EventTimer Pause Text 1 Text 2**

***Sequences:***

* Beamer HDMI 1 (PPP view)
* Audiochannel 1 fade up
* Audiochannel 2,3,4 fade down
* HDMI Switch channel 1 (Laptop PPP)
* Slidershow + Pause, Text 1 and Text 2

***Information for technician:***

1 B1 A1

***Execution text for PPP:***

JokiAutomation.exe "Pause" "Urheberrechtlich keine Liveübertragung" "Es geht in Kürze weiter"

**Band**

***Sequences:***

* Beamer HDMI 1 (PPP view)
* Audiochannel 2 (sumary) or 3 (room microphone) fade up
* Audiochannel 1,2 or 3,4 fade down
* HDMI Switch channel 1 (Laptop PPP)

***Information for technician:***

1 B1 A2

***Execution text for PPP:***

JokiAutomation.exe "Band"

**GoPro Actioncamera**

***Sequences:***

* Audiochannel 2 (sumary) or 3 (room microphone) fade up
* Audiochannel 1,2 or 3,4 fade down
* HDMI Switch channel 2 (GoPro)

***Information for technician:***

2 A2

***Execution text for PPP:***

JokiAutomation.exe "GoPro"

**Camcorder 1 (cam with position controller)**

***Sequences:***

* Audiochannel 2 (sumary) or 3 (room microphone) fade up
* Audiochannel 1,2 or 3,4 fade down
* HDMI Switch channel 3 (camcorder with position control)

***Information for technician:***

3 A2

***Execution text for PPP:***

JokiAutomation.exe "Altar"

**Camcorder 2 (preacher view)**

***Sequences:***

* Audiochannel 2 (sumary) or 3 (room microphone) fade up
* Audiochannel 1,2 or 3,4 fade down
* HDMI Switch channel 4 (camcorder 2 preacher view)

***Information for technician:***

4 A2

***Execution text for PPP:***

JokiAutomation.exe "Predigt"

**Prayer (prayer view)**

***Sequences:***

* Audiochannel 2 (sumary) or 3 (room microphone) fade up
* Audiochannel 1,2 or 3,4 fade down
* HDMI Switch channel 5 (combination PPP and GoPro)
* Beamer HDMI 1

***Information for technician:***

5 B1 A2

***Execution text for PPP:***

JokiAutomation.exe "Gebet"

**Audio sumary (sumary signal from amplifier)**

***Sequences:***

* Audiochannel 2 (sumary) fade up
* Audiochannel 1,3,4 fade down

***Information for technician:***

A2

***Execution text for PPP:***

JokiAutomation.exe "Audio\_Summensignal"

**Audio room (room micro from amplifier)**

***Sequences:***

* Audiochannel 3 (room microphone) fade up
* Audiochannel 1,2,4 fade down

***Information for technician:***

A3

***Execution text for PPP:***

JokiAutomation.exe "Audio\_RaumMikro"

**Audio channel 4 (channel 4 audiomix)**

***Sequences:***

* Audiochannel 4 fade up
* Audiochannel 1,2,3 fade down

***Information for technician:***

A4

***Execution text for PPP:***

JokiAutomation.exe "Audio\_Kanal4"

**Beamer PPP View**

***Sequences:***

* Switch beamer to HDMI 1 (Laptop PPP view)

***Information for technician:***

B1

***Execution text for PPP:***

JokiAutomation.exe "BEAMER\_PPP"

**Beamer PPP View**

***Sequences:***

* Switch beamer to HDMI 2 (Livestream - view)

***Information for technician:***

B2

***Execution text for PPP:***

JokiAutomation.exe "BEAMER\_LiveStream"

**Beamer Videoclip Text 1 Text 2**

***Sequences:***

* Beamer analog input
* Audiochannel 1 fade up
* Audiochannel 2,3,4 fade down
* HDMI Switch channel 1 (Laptop PPP)
* Pause, Text 1 and Text 2

***Information for technician:***

1 B3 A1

***Execution text for PPP:***

JokiAutomation.exe "BEAMER\_VideoClip" "Urheberrechtlich keine Liveübertragung" "Es geht in Kürze weiter"

**shut down sequence**

***Sequences:***

* Switch off Beamer
* Switch off HDMI switch
* Switch off backup recorder
* Shut down raspberry pi

***Information for technician:***

**Ausschaltsequenz!!!**

***Execution text for PPP:***

JokiAutomation.exe  "Ausschaltsequenz"